806
807
808
809
830
831
832
833
834
835
836
837
838
839
850
851
852
853
854
855
856
857
858
859
871
872
873
880
886
890
891
892
893
894
895
896
897
898
899
960
961
962
963
964
965
966
967
968
969
970
971
972
973
974
975
976
977
978

Nitwana, chaotism of

	-	Nitwana, chaotism of
	-	Nirwana chaotism of ~~

Nirwana, chaotism of 35~ ~ ú

	-	Nitwana, chaotism of X ~
	-	Nirwana, chaotism of ~ ~_, '_'
	-	Nirwana, chaotism of I

	-	Nirwana, chaotism of 	~

Nitwana, chaotism of J6 _~ _~_

	-	Nirwana, chaotism of X X
	-	Nirwana, chaotism of t_~ ~_~

Nirwana, chaotism o{

	-	Nirwana, chaotism of

	-	Nirwana, chaotism of	f. _~

		KOR Korea (Dem. People's Rep. of)
		- Nirwana, chaotism of ~ ~_r
	+8	HKG Hong-Kong
		Macao
	-	- Nirwana, chaotism of ~ ~ ]5 ~ ~~

		Dem. Kampuchea	~ ~+

LAO Lao Peoples Dem. Rep. < -

	-	-	Nirwana, chaotism of ~_	_
		-	Nirwana, chaotism of 	~J
	-	-	Nirwana, chaotism of

INMARSAT (Atlantic)~~ ~~

			INMARSAT (Pacific)	~_'

INMARSAT (Indian Ocean)

	+6	BGD Bangladesh (Peoples Rep. of)		ST:28~55 ~

	+8	TAI Taiwan ~ d_V~ _~~

	-	-	Nirwana, chaotism oI
	-	-	Nirwana, chaotism of ~_~ ~_r
		-	Nirwana, chaotism of
	-	-	Nirwana, chaotism of
	-	-	Nirwana, chaotism of ~ _~J'
	-	-	Nirwana, chaatism of ~4V Y
		-	Nirwana, chaotism of ~ ~_'
	-	-	Nirwana, chaotism of ~ ~ ~
	-	-	Nirwana, chaatism of ~ ~ QU
	-		Nirwana, chaotism of . ~ ~ ]5 ~ _~
	+5	MLD Maldives (Rep. oI) ~ ~ ~
	+2	LBN Lebanon	~~
	+2	JOR Jordan (Hashemite Kingdom of) ST: 10
	+2	SYR Syrian Arab Rep.

	+3	IRQ Iraq (Rep. of) ~ =~. _=J. ^`
	+3	KWT Kuwait (State of) ~C X

	+3	ARS Saudi Arabia (Kingdom of ~_	~_'
	+2	YEM Yemen Arab Rep.

	+4	OMA Oman (Sultanate of) ~ST:10	~f
		Yemen (People's Dem. Rep. of)

	-	- Nirwana, chaotism of ,~
	+4	UAE United Arab Emirates ~_	~_r

	+0	ISR Israel (State of) 	~SF: 3850'		1
	+3	BHR Bahr~in (State of) 	~_{	_

	+3	QAT Qatar (State of) ~V _~
		- Nirwana, chaotism of
		MNG Mongolian Peuples Rep., ~_r _
	+5.5	NPL Nepal

	-	Nirwana, chaotism of

. . .

_ _ _

001 Y ?
00 Y ?

00 ? ?
00, ? ?
00 ? ?
00 ? ?

		002 N ?

	?
	R2
	R2
	R2
	?
	?
	R2
	i
	?	00
	*?	00
	. 	~0
		o

00

y
y
N
N .
N ?
Y ?
N ?
N ?
y
?

?

N ?
? ?
Y ?
Y ?

?

	.	.	.

00 N ?

978 ?
979 ?
g90 ?
991 ?
992 ?
g93 ?
994 ~
995 ?
996 ?
,997 ?
998 ?
999 ?

Signalisierungsverfahren

~m inter-nat. Telefon7letzwerk de, Planeterl Erde
s~e es do~b .~\

frequencies in Hz, timing in ms, dbmO val-
ues are those of send level. Abkurzungser-
lauterungen siehe den entsprechenden Ar-
tikel hier sonstwo.

C3 (SF ~ 2280), C4(SF = 2040/2400
/ Toleranz ~ 6Hz / - 9dbM0 :~: 1)

Pulse & intervals between pulses 35 ~ 7ms,
binare Sigualobertragung; ~ ~ 2040,y Ä

	2400
	1	yyyx
	3	yyxx
	5	yxyx
	7	yxxx
	9	xyyx
	1 1	xyx~

EOP xxxx

C5 (SF = 2600/2400/SFT = 125
25ms/STisEOP)

	1	700+900
	3	900+1100
	5	900+1300
	7	700+1S00
	9	1100+1500
	11	700+1700
	KP1	1100+1700
	ST	1500+1700

xyyy
xyxy
~CXYV

Nirwana, chaotism of
Nirwana, chaotism of
Nirwana, chaatiem of
Nirwana, chaotism of œ
Nirwana, chaotism Of c
Nitwana, chaatism of
Nirwana, chaotism of
Nirwana, chaatism of
Nirwana, chaotism of
Nirwana, chaotism of ~
Nirwana, chaotism of ~c
Nirwana, chaotism of a

c, ~

E :`

0 ~
c

	R1	(SF	_	2600/2600/Toleranz

5Hz/ - 6 ~t ldBmO)
Pulees & intervels between pulBes 68
7ms/KP100 + 10ms/SF > 10m8

	1	700+900
	3	900+1100
	S	gOO+1300
	7	700+1500
	9	1100+1500
	11	700+1700
	KP1	1100+1700
	ST	1500+1700

R2 (SF = 3825/ - 11.5+ 1dvm01 KP2E
is KP2 with echo)

	1	1380+1500
	3	1500+1620
	5	1980+1740
	7	1380+1860
	9	1620+1860
	KP2E	1380+1980
	EOP	lB60+1980

SCTL (Socotel) (SF = 3850/PS >
35m5)
Dial-Freq. siehe C5. AS = 1900

Ls 16

	2	700+1100
	4	700+1300
	6	1100+1300
	8	900+1500
	0	1300+1500
	12	900+1700
	KP2	1500+1700

	2	700+1100
	4	700+1300
	6	1100+1300
	8	900+1S00
	0	1300+1500
	12	900+1700
	KP2	1300+1700

	2	1380+1620
	4	1380+1740
	6	1620+1740
	8	1500+1860
	0	17Js0+1860
	KP2	1500+1980

	L'~ ~nl~nPrlll~llh~r |	Das unssenschaftliche Fac~tt ft~r Datenreisendo	|	Seik 19 |

