			  
			       -- WAVY --
			 ----------------------
						 Released September 11,1994

 Copyright 1994 By ECLIPSE

Credits:
---------
  Code                  : LIGHT SHOW
  Code                  : HACKER CROLL
  Gfx                   : ZANY BIRD
  Gfx                   : SOOPL
  Gfx                   : TRACKS WOLF
  Music                 : REZ (AGOA)
  Music System Gravis   : RODDAN (CASCADA Use Gusplay Ver 1.5)
  Music System SBlaster : LIGHT SHOW (Use Diamond play Ver 0.51)
  Loader System         : LIGHT SHOW (Use E.O.S Ver 1.01)



Menbers Of ECLIPSE:
------------------
  Code        : LIGHT SHOW   (PC  386 DX 40  8Mo Ram  & AMIGA 500+)
  Code        : VIC          (PC  486 DX2 66 8Mo Ram  & AMIGA 500)
  Code        : HACKER CROLL (PC  486 DX 33  4Mo Ram  & APPLE II GS)
  Gfx         : SOOPL        (PC  486 DX2 66 16Mo Ram & AMIGA 500)
  Gfx         : ZANY BIRD    (AMIGA 1200 2Mo Ram)
  Gfx         : TRACKS WOLF  (PC  486 DX2 66 16Mo Ram & AMIGA 500)
  Music       : REZ          (AMIGA 1200 2Mo Ram)
  Distro      : AQUARIUM

Grettings:
-----------
  AGOA , ANARCHY , DISTORSION , EKO ST , FURTIVE , INFINY
  MEGABUSTER , TOXIC ZOMBIES ,ZUUL DESGIN

Contact Us:
------------
  If You Want To Contact Us For Something Write To:

  VIDAL Regis (LIGHT SHOW)
  Le Logis Neuf
  38780 ESTRABLIN
  FRANCE

Hardware Requirements:
-----------------------

  Processor     : 386 DX 33 Or Better

  Graphics card : VGA Card 100%. (Color And Mono)

  Music         : SoundBlaster (Pro)
		  Gravis Ultrasound

  Free memory   : 500000 Bytes


Information About The Music:
-----------------------------

  The Demo detect The Sound Blaster And The Gravis If it found in
  the AUTOEXEC.BAT :
    For Sound Blaster :

	     SET BLASTER = A220 I7 D1 T1
			     |   |  |  ===> 1 = Sound Blaster
			     |   |  |       2 = Sound Blaster Pro
			     |   |  |       3 = Sound Blaster 2.0
			     |   |  |       4 = Sound Blaster 16
			     |   |  |===> DMA Adress Of The SB
			     |   |===>Irq Of The SB
			     |===>Adress Of The SB

    For Gravis Ultrasnd :

	     SET ULTRASND = 220,1,1,7,7

	   !! The Gravis Must By In Port 220
				    irq 7
				    Dma 1


   Sorry For Not Use The Internal Speaker !!


			     <<<< END OF TEXT >>>>
