@X05cFos/2 professional v1.01       [iCE/uCF]
@X07Serial device driver that interfaces with
@X07ISDN CAPI 1.1 and 2.0 PDD.  Supports mul-
@X07tiple COM  ports simultaneously, control-
@X07led by a powerful AT command set. Virtual
@X07FOSSIL driver. Supports fast V.42bis data
@X07compression,  BTX, V.120, analogue modem,
@X07PPP Internet mode,  time synchronisation,
@X07X.31,  fax  command set,  dynamic channel
@X07bundling, more. Keyfile gener8tor incl.
@X03ÄÄÄÄĶ Üžßž iCEMAN & @X06tHE riDDLER ĶĶÄÄÄÄ
@X04   ÜÜÜ   ÜÜÜ    ÜÜÜÜ@X02ÜÜÜÜÜ    ÜÜÜÜÜÜÜÜÜ
@X04   ŪŪŪ   ŪŪŪ    ŪŪŪ @X02         ŪŪŪÜÜÜ
@X02   ŪŪŪÜ  ŪŪŪ    ŪŪŪÜ@X04         ŪŪŪ
@X02   ßßßßßßßßß    ßßßß@X04ßßßßß    ßßß
@X06ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ@X03ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ
@X02 u N I T E D  c R ’ C K I N G  f O R C E
@X05[oS2/cAPI fOSSIL dRIVER]ÄÄÄÄÄÄ[jUNE 1997]@X07
