         ________    ___  ____    _______    ________
       __\       \ _/   \/    \ _/       \ __\       \__
       \__   __   \\     \     \\   __    \\__   __   _/
        /    |/ __/           _/_   |/   _/_/    |/  /_
        \    /    \_           /    /      \          \
         \____\___//___\  /___/____________/\_____\___/
                        \/   redefine the future!

cross2 (final)
PC, 128 bytes intro

video - IlII, suedon
code reverse - IlII
new code - IlII
ascii - namd

farted by ded

This is a reimagining of the iconic cross1 by Queue Members
Group (Russia, Samara), which came 1st at Demodesign contest 
back in 1996. Original work was compiled on 08-08-1996 and 
was submitted to Demodesign compo as 128 bytes intro but in 
fact it's 126 bytes long.

Also you can check some photos from the Enlight'96. There 
you'll find a T-shirt with hex dump of this masterpiece intro 
on the back. T-shirts and photos was done by organizers of 
Demodesign and Enlight to popularize ideas of PC sizecoding.

A cross was optimized (all of the text output, color and sound)
into a cross2 (final) in march 2020 by IlII (Russia, Samara).

official QMG web-site: http://qmg.org
official QMG download directory: http://qmg.org/files/demos/qmg
cross1 on Pouet: https://www.pouet.net/prod.php?which=6212

cross1 and cross2 (final) on YouTube in glorious 4320p60 8K: 

cross1 https://www.youtube.com/watch?v=nkaWruHO4BU
cross2 https://www.youtube.com/watch?v=2EHkV7eFwEI

official Demodesign'96 pack: 
https://files.scene.org/view/parties/1996/demodesign96/128b/128-all.zip

Please note that when you'll compile cross.asm it's not going to be 
byte-by-byte identical to original .com file. 

The reason for that is simple. For example:

mov cx,ax

can be encoded as

8B C8
or
89 C1

ñatch it?

---[original cross1 nfo]---
128 byte intro by Mad Max / Queue Members Group
coded for DEMO.DESIGN contest                  
welcome to SU.SATANISM ;-) 
---------------------------

RMDA @ https://rmda.su 15-03-2020

russkie idut...