Kumiakku - Rubber Battery
a tAAt 2002 demo
-------------------------

INSTALLING THE DEMO TO YOPY YDK-1000 (or YP3000)

Transfer the file kumiakku.tar.gz to the device. You can use some file
transfer utility which is provided with Yopy, or you can use a
terminal software to connect to the device via serial port and use
e.g. ZModem to transfer the file.

The demo needs about 1350 KB storage space and a few megabytes of
runtime memory (less than 8 MB is enough).
 
Here is instructions how to transfer the file with terminal software:

1. Connect the device to a serial port.
2. Open 115200 8N1 connection to the serial port you are using.
3. Press enter, if you have succeeded you should see the login prompt.
   Below is list of the actions you should do. For lines which start
   with an asterisk ('*') first column is the prompt what the PDA
   prints and second column is what you should write.
   * yopy login:                    root
   * [root@yopy /root]#             cd /tmp
   * [root@yopy /tmp]#              rz
   At this point start sending the file "kumiakku.tar.gz" with your
   terminal software using ZModem transfer protocol.
   * [root@yopy /tmp]#              tar Pzxf kumiakku.tar.gz
   Uncompressing the demo takes a while..
   * [root@yopy /tmp]#              rm kumiakku.tar.gz
   * [root@yopy /tmp]#              logout
   After this you should get the login prompt again.
4. Now the demo should be ready to run! Open the application launch
   menu and select Graphics->Kumiakku to run the demo.


To uninstall the demo, remove directory "/kumiakku" and file
"/usr/local/share/gnome/apps/Graphics/kumiakku.desktop" in the device.
