[renderBuffer]
id 101
start 58
end 73
enabled 1
layer 24
blend SRC_ALPHA ONE
; Recovers ta previously saved screen buffer from the video
; card and puts it on the screen with the desired parameters

; Integer representing the texture unit that will be
; recovered over the current screen contents (0 to 9)
; if '-1' is passed, no texture is binded (useful for glsl)
param 3

; Clear the screen buffer before restoring? (1=yes, 0=no)
fClearScreenBuffer 0

; Clear the depth buffer after restoring? (1=yes, 0=no)
fClearDepthBuffer 0

; Fullscreen restore? 0 = no; 1 = yes
fFullScreenRestore 1