THE FLATTER by CASTOR of INVERSION

Actual size is of executable is 15041 bytes divided in three blocks of 1766, 9477 and 3798 bytes. The rest of the rom is zero-padded.
For ROM to be playable on real hardware the minimum ROM size is 32kB, accompanied by on-cartridge RAM of similar size.