res: 159,       // pads: reset
rw: 1156,       // pads: read not write
db0: 1005,      // pads: databus
db1: 82,
db2: 945,
db3: 650,
db4: 1393,
db5: 175,
db6: 1591,
db7: 1349,
ab0: 268,       // pads: address bus
ab1: 451,
ab2: 1340,
ab3: 211,
ab4: 435,
ab5: 736,
ab6: 887,
ab7: 1493,
ab8: 230,
ab9: 148,
ab10: 1443,
ab11: 399,
ab12: 1237,
ab13: 349,
ab14: 672,
ab15: 195,
sync: 539,      // pads
so: 1672,       // pads: set overflow
clk0: 1171,     // pads
clk1out: 1163,  // pads
clk2out: 421,   // pads
rdy: 89,        // pads: ready
nmi: 1297,      // pads: non maskable interrupt
irq: 103,       // pads
vcc: 657,       // pads
vss: 558,       // pads
a0: 737,        // machine state: accumulator
a1: 1234,
a2: 978,
a3: 162,
a4: 727,
a5: 858,
a6: 1136,
a7: 1653,
y0: 64,         // machine state: y index register
y1: 1148,
y2: 573,
y3: 305,
y4: 989,
y5: 615,
y6: 115,
y7: 843,
x0: 1216,       // machine state: x index register
x1: 98,
x2: 1,
x3: 1648,
x4: 85,
x5: 589,
x6: 448,
x7: 777,
pcl0: 1139,     // machine state: program counter low (first storage node output)
pcl1: 1022,
pcl2: 655,
pcl3: 1359,
pcl4: 900,
pcl5: 622,
pcl6: 377,
pcl7: 1611,
pclp0: 488,    // machine state: program counter low (pre-incremented?, second storage node)
pclp1: 976,
pclp2: 481,
pclp3: 723,
pclp4: 208,
pclp5: 72,
pclp6: 1458,
pclp7: 1647,
"#pclp0": 1227,    // machine state: program counter low (pre-incremented?, inverse second storage node)
"~pclp0": 1227,     // automatic alias replacing hash with tilde
"#pclp1": 1102,
"~pclp1": 1102, // automatic alias replacing hash with tilde
"#pclp2": 1079,
"~pclp2": 1079, // automatic alias replacing hash with tilde
"#pclp3": 868,
"~pclp3": 868, // automatic alias replacing hash with tilde
"#pclp4": 39,
"~pclp4": 39, // automatic alias replacing hash with tilde
"#pclp5": 1326,
"~pclp5": 1326, // automatic alias replacing hash with tilde
"#pclp6": 731,
"~pclp6": 731, // automatic alias replacing hash with tilde
"#pclp7": 536,
"~pclp7": 536, // automatic alias replacing hash with tilde
pch0: 1670,     // machine state: program counter high (first storage node)
pch1: 292,
pch2: 502,
pch3: 584,
pch4: 948,
pch5: 49,
pch6: 1551,
pch7: 205,
pchp0: 1722,     // machine state: program counter high (pre-incremented?, second storage node output)
pchp1: 209,
pchp2: 1496,
pchp3: 141,
pchp4: 27,
pchp5: 1301,
pchp6: 652,
pchp7: 1206,
"#pchp0": 780,     // machine state: program counter high (pre-incremented?, inverse second storage node)
"~pchp0": 780,      // automatic alias replacing hash with tilde
"#pchp1": 113,
"~pchp1": 113, // automatic alias replacing hash with tilde
"#pchp2": 114,
"~pchp2": 114, // automatic alias replacing hash with tilde
"#pchp3": 124,
"~pchp3": 124, // automatic alias replacing hash with tilde
"#pchp4": 820,
"~pchp4": 820, // automatic alias replacing hash with tilde
"#pchp5": 33,
"~pchp5": 33, // automatic alias replacing hash with tilde
"#pchp6": 751,
"~pchp6": 751, // automatic alias replacing hash with tilde
"#pchp7": 535,
"~pchp7": 535, // automatic alias replacing hash with tilde
p0: 32,         // C bit of status register (storage node)
p1: 627,        // Z bit of status register (storage node)
p2: 1553,       // I bit of status register (storage node)
p3: 348,        // D bit of status register (storage node)
p4: 1119,       // there is no bit4 in the status register! (not a storage node)
p5: -1,         // there is no bit5 in the status register! (not a storage node)
p6: 77,         // V bit of status register (storage node)
p7: 1370,       // N bit of status register (storage node)
Pout0: 687,
Pout1: 1444,
Pout2: 1421,
Pout3: 439,
Pout4: 1119,    // there is no bit4 in the status register!
Pout5: -1,      // there is no bit5 in the status register!
Pout6: 77,
Pout7: 1370,
s0: 1403,       // machine state: stack pointer
s1: 183,
s2: 81,
s3: 1532,
s4: 1702,
s5: 1098,
s6: 1212,
s7: 1435,
ir0: 328,       // internal state: instruction register
ir1: 1626,
ir2: 1384,
ir3: 1576,
ir4: 1112,
ir5: 1329,      // ir5 distinguishes branch set from branch clear
ir6: 337,
ir7: 1328,
notir0: 194,    // internal signal: instruction register inverted outputs
notir1: 702,
notir2: 1182,  
notir3: 1125,  
notir4: 26,
notir5: 1394,
notir6: 895,
notir7: 1320,
irline3: 996,   // internal signal: PLA input - ir0 OR ir1
clock1: 1536,   // internal state: timing control aka #T0
clock1: 1536,    // automatic alias replacing hash with tilde
clock2: 156,    // internal state: timing control aka #T+
clock2: 156,     // automatic alias replacing hash with tilde
t2: 971,        // internal state: timing control
t3: 1567,
t4: 690,
t5: 909,
noty0: 1025,    // datapath state: not Y register
noty1: 1138,
noty2: 1484,
noty3: 184,
noty4: 565,
noty5: 981,
noty6: 1439,
noty7: 1640,
notx0: 987,     // datapath state: not X register
notx1: 1434,
notx2: 890,
notx3: 1521,
notx4: 485,
notx5: 1017,
notx6: 730,
notx7: 1561,
nots0: 418,     // datapath state: not stack pointer
nots1: 1064,
nots2: 752,
nots3: 828,
nots4: 1603,
nots5: 601,
nots6: 1029,
nots7: 181,
notidl0: 116,   // datapath state: internal data latch (first storage node)
notidl1: 576,
notidl2: 1485,
notidl3: 1284,
notidl4: 1516,
notidl5: 498,
notidl6: 1537,
notidl7: 529,
idl0: 1597,     // datapath signal: internal data latch (driven output)
idl1: 870,
idl2: 1066,
idl3: 464,
idl4: 1306,
idl5: 240,
idl6: 1116,
idl7: 391,
sb0: 54,        // datapath bus: special bus
sb1: 1150,
sb2: 1287,
sb3: 1188,
sb4: 1405,
sb5: 166,
sb6: 1336,
sb7: 1001,
notalu0: 394,   // datapath state: alu output storage node (inverse) aka #ADD0
notalu0: 394,    // automatic alias replacing hash with tilde
notalu1: 697,
notalu2: 276,
notalu3: 495,
notalu4: 1490,
notalu5: 893,
notalu6: 68,
notalu7: 1123,
alu0: 401,      // datapath signal: ALU output aka ADD0out
alu1: 872,
alu2: 1637,
alu3: 1414,
alu4: 606,
alu5: 314,
alu6: 331,
alu7: 765,
dasb0: 54,      // same node as sb0
dasb1: 1009,
dasb2: 450,
dasb3: 1475,
dasb4: 1405,    // same node as sb4
dasb5: 263,
dasb6: 679,
dasb7: 1494,
adl0: 413,      // internal bus: address low
adl1: 1282,
adl2: 1242,
adl3: 684,
adl4: 1437,
adl5: 1630,
adl6: 121,
adl7: 1299,
adh0: 407,      // internal bus: address high
adh1: 52,
adh2: 1651,
adh3: 315,
adh4: 1160,
adh5: 483,
adh6: 13,
adh7: 1539,
idb0: 1108,     // internal bus: data bus
idb1: 991,
idb2: 1473,
idb3: 1302,
idb4: 892,
idb5: 1503,
idb6: 833,
idb7: 493,
notdor0: 222,   // internal state: data output register (storage node)
notdor1: 527,
notdor2: 1288,
notdor3: 823,
notdor4: 873,
notdor5: 1266,
notdor6: 1418,
notdor7: 158,
dor0: 97,       // internal signal: data output register
dor1: 746,
dor2: 1634,
dor3: 444,
dor4: 1088,
dor5: 1453,
dor6: 1415,
dor7: 63,
"pd0.clearIR": 1622,       // internal state: predecode register output (anded with not ClearIR)
"pd1.clearIR": 809,
"pd2.clearIR": 1671,
"pd3.clearIR": 1587,
"pd4.clearIR": 540,
"pd5.clearIR": 667,
"pd6.clearIR": 1460,
"pd7.clearIR": 1410,
pd0: 758,       // internal state: predecode register (storage node)
pd1: 361,
pd2: 955,
pd3: 894,
pd4: 369,
pd5: 829,
pd6: 1669,
pd7: 1690,
"PD-xxxx10x0": 1019,
"PD-1xx000x0": 1294,
"PD-0xx0xx0x": 365,
"PD-xxx010x1": 302,
"PD-n-0xx0xx0x": 125,
"#TWOCYCLE": 851,
"~TWOCYCLE": 851, // automatic alias replacing hash with tilde
"#TWOCYCLE.phi1": 792,
"~TWOCYCLE.phi1": 792, // automatic alias replacing hash with tilde
"ONEBYTE": 778,
abl0: 1096,     // internal bus: address bus low latched data out (inverse of inverted storage node)
abl1: 376,
abl2: 1502,
abl3: 1250,
abl4: 1232,
abl5: 234,
abl6: 178,
abl7: 567,
"#ABL0": 153,   // internal state: address bus low latched data out (storage node, inverted)
"~ABL0": 153,    // automatic alias replacing hash with tilde
"#ABL1": 107,
"~ABL1": 107, // automatic alias replacing hash with tilde
"#ABL2": 707,
"~ABL2": 707, // automatic alias replacing hash with tilde
"#ABL3": 825,
"~ABL3": 825, // automatic alias replacing hash with tilde
"#ABL4": 364,
"~ABL4": 364, // automatic alias replacing hash with tilde
"#ABL5": 1513,
"~ABL5": 1513, // automatic alias replacing hash with tilde
"#ABL6": 1307,
"~ABL6": 1307, // automatic alias replacing hash with tilde
"#ABL7": 28,
"~ABL7": 28, // automatic alias replacing hash with tilde
abh0: 1429,     // internal bus: address bus high latched data out (inverse of inverted storage node)
abh1: 713,
abh2: 287,
abh3: 422,
abh4: 1143,
abh5: 775,
abh6: 997,
abh7: 489,
"#ABH0": 1062,  // internal state: address bus high latched data out (storage node, inverted)
"~ABH0": 1062,   // automatic alias replacing hash with tilde
"#ABH1": 907,
"~ABH1": 907, // automatic alias replacing hash with tilde
"#ABH2": 768,
"~ABH2": 768, // automatic alias replacing hash with tilde
"#ABH3": 92,
"~ABH3": 92, // automatic alias replacing hash with tilde
"#ABH4": 668,
"~ABH4": 668, // automatic alias replacing hash with tilde
"#ABH5": 1128,
"~ABH5": 1128, // automatic alias replacing hash with tilde
"#ABH6": 289,
"~ABH6": 289, // automatic alias replacing hash with tilde
"#ABH7": 429,
"~ABH7": 429, // automatic alias replacing hash with tilde
"branch-back": 626,           // distinguish forward from backward branches
"branch-forward.phi1": 1110,  // distinguish forward from backward branches
"branch-back.phi1": 771,      // distinguish forward from backward branches in IPC logic
notRdy0: 248,           // internal signal: global pipeline control
"notRdy0.phi1": 1272,   // delayed pipeline control
"notRdy0.delay": 770,   // global pipeline control latched by phi1 and then phi2
"#notRdy0.delay": 559,  // global pipeline control latched by phi1 and then phi2 (storage node)
"~notRdy0.delay": 559,   // automatic alias replacing hash with tilde
Reset0: 67,     // internal signal: retimed reset from pin
C1x5Reset: 926, // retimed and pipelined reset in progress
notRnWprepad: 187, // internal signal: to pad, yet to be inverted and retimed
RnWstretched: 353, // internal signal: control datapad output drivers, aka TRISTATE
"#DBE": 1035,      // internal signal: formerly from DBE pad (6501)
"~DBE": 1035,       // automatic alias replacing hash with tilde
cp1: 710,       // internal signal: clock phase 1
cclk: 943,      // unbonded pad: internal non-overlappying phi2
fetch: 879,     // internal signal
clearIR: 1077,  // internal signal
H1x1: 1042,     // internal signal: drive status byte onto databus
"op-sty/cpy-mem": 1601,        // pla0
"op-T3-ind-y": 60,             // pla1
"op-T2-abs-y": 1512,           // pla2
"op-T0-iny/dey": 382,          // pla3
"x-op-T0-tya": 1173,           // pla4
"op-T0-cpy/iny": 1233,         // pla5
"op-T2-idx-x-xy": 258,         // pla6
"op-xy": 1562,                 // pla7
"op-T2-ind-x": 84,             // pla8
"x-op-T0-txa": 1543,           // pla9
"op-T0-dex": 76,               // pla10
"op-T0-cpx/inx": 1658,         // pla11
"op-from-x": 1540,             // pla12
"op-T0-txs": 245,              // pla13
"op-T0-ldx/tax/tsx": 985,      // pla14
"op-T+-dex": 786,              // pla15
"op-T+-inx": 1664,             // pla16
"op-T0-tsx": 682,              // pla17
"op-T+-iny/dey": 1482,         // pla18
"op-T0-ldy-mem": 665,          // pla19
"op-T0-tay/ldy-not-idx": 286,  // pla20
"op-T0-jsr": 271,              // pla21
"op-T5-brk": 370,              // pla22
"op-T0-php/pha": 552,          // pla23
"op-T4-rts": 1612,             // pla24
"op-T3-plp/pla": 1487,         // pla25
"op-T5-rti": 784,              // pla26
"op-ror": 244,                 // pla27
"op-T2": 788,                  // pla28
"op-T0-eor": 1623,             // pla29
"op-jmp": 764,                 // pla30
"op-T2-abs": 1057,             // pla31
"op-T0-ora": 403,              // pla32
"op-T2-ADL/ADD":204,           // pla33 
"op-T0":1273,                  // pla34 
"op-T2-stack":1582,            // pla35 
"op-T3-stack/bit/jmp":1031,    // pla36 
"op-T4-brk/jsr":804,           //  pla37
"op-T4-rti":1311,              //  pla38
"op-T3-ind-x":1428,            //  pla39
"op-T4-ind-y":492,             //  pla40
"op-T2-ind-y":1204,            //  pla41
"op-T3-abs-idx":58,            //  pla42
"op-plp/pla":1520,             //  pla43
"op-inc/nop":324,              //  pla44
"op-T4-ind-x":1259,            //  pla45
"x-op-T3-ind-y":342,           //  pla46
"op-rti/rts":857,              //  pla47
"op-T2-jsr":712,               //  pla48
"op-T0-cpx/cpy/inx/iny":1337,  //  pla49
"op-T0-cmp":1355,              //  pla50
"op-T0-sbc":787,               //  pla51   //  52:111XXXXX  1  0  T0SBC
"op-T0-adc/sbc":575,           //  pla52   //  51:X11XXXXX  1  0  T0ADCSBC
"op-rol/ror":1466,             //  pla53
"op-T3-jmp":1381,              //  pla54
"op-shift":546,                //  pla55
"op-T5-jsr":776,               //  pla56
"op-T2-stack-access":157,      //  pla57
"op-T0-tya":257,               //  pla58
"op-T+-ora/and/eor/adc":1243,  //  pla59
"op-T+-adc/sbc":822,           //  pla60
"op-T+-shift-a":1324,          //  pla61
"op-T0-txa":179,               //  pla62
"op-T0-pla":131,               //  pla63
"op-T0-lda":1420,              //  pla64
"op-T0-acc":1342,              //  pla65
"op-T0-tay":4,                 //  pla66
"op-T0-shift-a":1396,          //  pla67
"op-T0-tax":167,               //  pla68
"op-T0-bit":303,               //  pla69
"op-T0-and":1504,              //  pla70
"op-T4-abs-idx":354,           //  pla71
"op-T5-ind-y":1168,            //  pla72
"op-branch-done":1721,         //  pla73    // has extra non-pla input
"op-T2-pha":1086,              //  pla74
"op-T0-shift-right-a":1074,    //  pla75
"op-shift-right":1246,         //  pla76
"op-T2-brk":487,               //  pla77
"op-T3-jsr":579,               //  pla78
"op-sta/cmp":145,              //  pla79
"op-T2-branch":1239,           //  pla80      //  T2BR, 83 for Balazs
"op-T2-zp/zp-idx":285,         //  pla81
"op-T2-ind":1524,              //  pla82
"op-T2-abs-access":273,        //  pla83      // has extra pulldown: pla97
"op-T5-rts":0,                 //  pla84
"op-T4":341,                   //  pla85
"op-T3":120,                   //  pla86
"op-T0-brk/rti":1478,          //  pla87
"op-T0-jmp":594,               //  pla88
"op-T5-ind-x":1210,            //  pla89
"op-T3-abs/idx/ind":677,       //  pla90      // has extra pulldown: pla97
"x-op-T4-ind-y":461,           //  pla91
"x-op-T3-abs-idx":447,         //  pla92
"op-T3-branch":660,            //  pla93
"op-brk/rti":1557,             //  pla94
"op-jsr":259,                  //  pla95
"x-op-jmp":1052,               //  pla96
"op-push/pull":791,            //  pla97      // feeds into pla83 and pla90 (no normal pla output)
"op-store":517,                //  pla98
"op-T4-brk":352,               //  pla99
"op-T2-php":750,               //  pla100
"op-T2-php/pha":932,           //  pla101
"op-T4-jmp":1589,              //  pla102
"op-T5-rti/rts":446,           //  pla103
"xx-op-T5-jsr":528,            //  pla104
"op-T2-jmp-abs":309,           //  pla105
"x-op-T3-plp/pla":1430,        //  pla106
"op-lsr/ror/dec/inc":53,       //  pla107
"op-asl/rol":691,              //  pla108
"op-T0-cli/sei":1292,          //  pla109
"op-T+-bit":1646,              //  pla110
"op-T0-clc/sec":1114,          //  pla111
"op-T3-mem-zp-idx":904,        //  pla112
"x-op-T+-adc/sbc":1155,        //  pla113
"x-op-T0-bit":1476,            //  pla114
"op-T0-plp":1226,              //  pla115
"x-op-T4-rti":1569,            //  pla116
"op-T+-cmp":301,               //  pla117
"op-T+-cpx/cpy-abs":950,       //  pla118
"op-T+-asl/rol-a":1665,        //  pla119
"op-T+-cpx/cpy-imm/zp":1710,   //  pla120
"x-op-push/pull":1050,         //  pla121    // feeds into pla130 (no normal pla output)
"op-T0-cld/sed":1419,          //  pla122
"#op-branch-bit6":840,         //  pla123    // IR bit6 used only to detect branch type
"~op-branch-bit6":840,          // automatic alias replacing hash with tilde
"op-T3-mem-abs":607,           //  pla124
"op-T2-mem-zp":219,            //  pla125
"op-T5-mem-ind-idx":1385,      //  pla126
"op-T4-mem-abs-idx":281,       //  pla127
"#op-branch-bit7":1174,        //  pla128    // IR bit7 used only to detect branch type
"~op-branch-bit7":1174,         // automatic alias replacing hash with tilde
"op-clv":1164,                 //  pla129
"op-implied":1006,             //  pla130    // has extra pulldowns: pla121 and ir0
"#op-branch-done": 1048,
"~op-branch-done": 1048, // automatic alias replacing hash with tilde
"#op-T3-branch": 1708,
"~op-T3-branch": 1708, // automatic alias replacing hash with tilde
"op-ANDS": 1228,
"op-EORS": 1689,
"op-ORS": 522,
"op-SUMS": 1196,
"op-SRS": 934,
"#op-store": 925,
"~op-store": 925, // automatic alias replacing hash with tilde
"#WR": 1352,
"~WR": 1352, // automatic alias replacing hash with tilde
"op-rmw": 434,
"short-circuit-idx-add": 1185,
"short-circuit-branch-add": 430,
"#op-set-C": 252,
"~op-set-C": 252, // automatic alias replacing hash with tilde
nnT2BR: 967,    // doubly inverted
BRtaken: 1544,  // aka #TAKEN
BRtaken: 1544,   // automatic alias replacing hash with tilde
IRQP: 675,
"#IRQP": 888,
"~IRQP": 888, // automatic alias replacing hash with tilde
NMIP: 1032,
"#NMIP": 297,
"~NMIP": 297, // automatic alias replacing hash with tilde
"#NMIG": 264,
"~NMIG": 264, // automatic alias replacing hash with tilde
NMIL: 1374,
RESP: 67,
RESG: 926,
VEC0: 1465,
VEC1: 1481,
"#VEC": 1134,
"~VEC": 1134, // automatic alias replacing hash with tilde
D1x1: 827,         // internal signal: interrupt handler related
"brk-done": 1382,  // internal signal: interrupt handler related
INTG: 1350,        // internal signal: interrupt handler related
"pipe#VEC": 1431,     // latched #VEC
"pipe~VEC": 1431,      // automatic alias replacing hash with tilde
"pipeT-SYNC": 537,
pipeT2out: 40,
pipeT3out: 706,
pipeT4out: 1373,
pipeT5out: 940,
pipeIPCrelated: 832,
pipeUNK01: 1530,
pipeUNK02: 974,
pipeUNK03: 1436,
pipeUNK04: 99,
pipeUNK05: 44,
pipeUNK06: 443,
pipeUNK07: 215,
pipeUNK08: 338,
pipeUNK09: 199,
pipeUNK10: 215,
pipeUNK11: 1011,
pipeUNK12: 1283,
pipeUNK13: 1442,
pipeUNK14: 1607,
pipeUNK15: 1577, // inverse of H1x1, write P onto idb (PHP, interrupt)
pipeUNK16: 1051,
pipeUNK17: 1078,
pipeUNK18: 899,
pipeUNK19: 832,
pipeUNK20: 294,
pipeUNK21: 1176,
pipeUNK22: 561, // becomes dpc22
pipeUNK23: 596,
pipephi2Reset0: 449,
pipephi2Reset0x: 1036, // a second copy of the same latch
pipeUNK26: 1321,
pipeUNK27: 73,
pipeUNK28: 685,
pipeUNK29: 1008,
pipeUNK30: 1652,
pipeUNK31: 614,
pipeUNK32: 960,
pipeUNK33: 848,
pipeUNK34: 56,
pipeUNK35: 1713,
pipeUNK36: 729,
pipeUNK37: 197,
"pipe#WR.phi2": 1131,
"pipe~WR.phi2": 1131, // automatic alias replacing hash with tilde
pipeUNK39: 151,
pipeUNK40: 456,
pipeUNK41: 1438,
pipeUNK42: 1104,
"pipe#T0": 554,   // aka #T0.phi2
"pipe~T0": 554,    // automatic alias replacing hash with tilde
pipeVectorA0: 357,
pipeVectorA1: 170,
pipeVectorA2: 45,
"0/ADL0": 217,
"0/ADL1": 686,
"0/ADL2": 1193,
pipedpc28: 683,
alua0: 1167,
alua1: 1248,
alua2: 1332,
alua3: 1680,
alua4: 1142,
alua5: 530,
alua6: 1627,
alua7: 1522,
alub0: 977,
alub1: 1432,
alub2: 704,
alub3: 96,
alub4: 1645,
alub5: 1678,
alub6: 235,
alub7: 1535,
C01: 1285,
C12: 505,
C23: 1023,
C34: 78,
C45: 142,
C56: 500,
C67: 1314,
C78: 808,
"C78.phi2": 560,
DC34: 1372,   // lower nibble decimal carry
DC78: 333,    // carry for decimal mode
"DC78.phi2": 164,
"#C01": 1506,
"~C01": 1506, // automatic alias replacing hash with tilde
"#C12": 1122,
"~C12": 1122, // automatic alias replacing hash with tilde
"#C23": 1003,
"~C23": 1003, // automatic alias replacing hash with tilde
"#C34": 1425,
"~C34": 1425, // automatic alias replacing hash with tilde
"#C45": 1571,
"~C45": 1571, // automatic alias replacing hash with tilde
"#C56": 427,
"~C56": 427, // automatic alias replacing hash with tilde
"#C67": 592,
"~C67": 592, // automatic alias replacing hash with tilde
"#C78": 1327,
"~C78": 1327, // automatic alias replacing hash with tilde
"DA-C01": 623,
"DA-AB2": 216,
"DA-AxB2": 516,
"DA-C45": 1144,
"#DA-ADD1": 901,
"~DA-ADD1": 901, // automatic alias replacing hash with tilde
"#DA-ADD2": 699,
"~DA-ADD2": 699, // automatic alias replacing hash with tilde
"#(AxBxC)0": 371,
"~(AxBxC)0": 371, // automatic alias replacing hash with tilde
"#(AxBxC)1": 965,
"~(AxBxC)1": 965, // automatic alias replacing hash with tilde
"#(AxBxC)2": 22,
"~(AxBxC)2": 22, // automatic alias replacing hash with tilde
"#(AxBxC)3": 274,
"~(AxBxC)3": 274, // automatic alias replacing hash with tilde
"#(AxBxC)4": 651,
"~(AxBxC)4": 651, // automatic alias replacing hash with tilde
"#(AxBxC)5": 486,
"~(AxBxC)5": 486, // automatic alias replacing hash with tilde
"#(AxBxC)6": 1197,
"~(AxBxC)6": 1197, // automatic alias replacing hash with tilde
"#(AxBxC)7": 532,
"~(AxBxC)7": 532, // automatic alias replacing hash with tilde
AxB1: 425,
AxB3: 640,
AxB5: 1220,
AxB7: 1241,
"#(AxB)0": 1525,
"~(AxB)0": 1525, // automatic alias replacing hash with tilde
"#(AxB)2": 701,
"~(AxB)2": 701, // automatic alias replacing hash with tilde
"#(AxB)4": 308,
"~(AxB)4": 308, // automatic alias replacing hash with tilde
"#(AxB)6": 1459,
"~(AxB)6": 1459, // automatic alias replacing hash with tilde
"(AxB)0.#C0in": 555,
"(AxB)0.~C0in": 555, // automatic alias replacing hash with tilde
"(AxB)2.#C12": 193,
"(AxB)2.~C12": 193, // automatic alias replacing hash with tilde
"(AxB)4.#C34": 65,
"(AxB)4.~C34": 65, // automatic alias replacing hash with tilde
"(AxB)6.#C56": 174,
"(AxB)6.~C56": 174, // automatic alias replacing hash with tilde
"#(AxB1).C01": 295,
"~(AxB1).C01": 295, // automatic alias replacing hash with tilde
"#(AxB3).C23": 860,
"~(AxB3).C23": 860, // automatic alias replacing hash with tilde
"#(AxB5).C45": 817,
"~(AxB5).C45": 817, // automatic alias replacing hash with tilde
"#(AxB7).C67": 1217,
"~(AxB7).C67": 1217, // automatic alias replacing hash with tilde
"#A.B0": 1628,
"~A.B0": 1628, // automatic alias replacing hash with tilde
"#A.B1": 841,
"~A.B1": 841, // automatic alias replacing hash with tilde
"#A.B2": 681,
"~A.B2": 681, // automatic alias replacing hash with tilde
"#A.B3": 350,
"~A.B3": 350, // automatic alias replacing hash with tilde
"#A.B4": 1063,
"~A.B4": 1063, // automatic alias replacing hash with tilde
"#A.B5": 477,
"~A.B5": 477, // automatic alias replacing hash with tilde
"#A.B6": 336,
"~A.B6": 336, // automatic alias replacing hash with tilde
"#A.B7": 1318,
"~A.B7": 1318, // automatic alias replacing hash with tilde
"A+B0": 693,
"A+B1": 1021,
"A+B2": 110,
"A+B3": 1313,
"A+B4": 918,
"A+B5": 1236,
"A+B6": 803,
"A+B7": 117,
"#(A+B)0": 143,
"~(A+B)0": 143, // automatic alias replacing hash with tilde
"#(A+B)1": 155,
"~(A+B)1": 155, // automatic alias replacing hash with tilde
"#(A+B)2": 1691,
"~(A+B)2": 1691, // automatic alias replacing hash with tilde
"#(A+B)3": 649,
"~(A+B)3": 649, // automatic alias replacing hash with tilde
"#(A+B)4": 404,
"~(A+B)4": 404, // automatic alias replacing hash with tilde
"#(A+B)5": 1632,
"~(A+B)5": 1632, // automatic alias replacing hash with tilde
"#(A+B)6": 1084,
"~(A+B)6": 1084, // automatic alias replacing hash with tilde
"#(A+B)7": 1398,
"~(A+B)7": 1398, // automatic alias replacing hash with tilde
"#(AxB)0": 1525,
"~(AxB)0": 1525, // automatic alias replacing hash with tilde
"#(AxB)2": 701,
"~(AxB)2": 701, // automatic alias replacing hash with tilde
"#(AxB)4": 308,
"~(AxB)4": 308, // automatic alias replacing hash with tilde
"#(AxB)6": 1459,
"~(AxB)6": 1459, // automatic alias replacing hash with tilde
"#(AxB)1": 953,
"~(AxB)1": 953, // automatic alias replacing hash with tilde
"#(AxB)3": 884,
"~(AxB)3": 884, // automatic alias replacing hash with tilde
"#(AxB)5": 1469,
"~(AxB)5": 1469, // automatic alias replacing hash with tilde
"#(AxB)7": 177,
"~(AxB)7": 177, // automatic alias replacing hash with tilde
"#aluresult0": 957,   // alu result latch input
"~aluresult0": 957,    // automatic alias replacing hash with tilde
"#aluresult1": 250,
"~aluresult1": 250, // automatic alias replacing hash with tilde
"#aluresult2": 740,
"~aluresult2": 740, // automatic alias replacing hash with tilde
"#aluresult3": 1071,
"~aluresult3": 1071, // automatic alias replacing hash with tilde
"#aluresult4": 296,
"~aluresult4": 296, // automatic alias replacing hash with tilde
"#aluresult5": 277,
"~aluresult5": 277, // automatic alias replacing hash with tilde
"#aluresult6": 722,
"~aluresult6": 722, // automatic alias replacing hash with tilde
"#aluresult7": 304,
"~aluresult7": 304, // automatic alias replacing hash with tilde
"ADL/ABL": 639,      // load ABL latches from ADL bus
"ADH/ABH": 821,      // load ABH latches from ADH bus
dpc0_YSB: 801,       // drive sb from y
dpc1_SBY: 325,       // load y from sb
dpc2_XSB: 1263,      // drive sb from x
dpc3_SBX: 1186,      // load x from sb
dpc4_SSB: 1700,      // drive sb from stack pointer
dpc5_SADL: 1468,     // drive adl from stack pointer
dpc6_SBS: 874,       // load stack pointer from sb
dpc7_SS: 654,        // recirculate stack pointer
dpc8_nDBADD: 1068,   // alu b side: select not-idb input
dpc9_DBADD: 859,     // alu b side: select idb input
dpc10_ADLADD: 437,   // alu b side: select adl input
dpc11_SBADD: 549,    // alu a side: select sb
dpc12_0ADD: 984,     // alu a side: select zero
dpc13_ORS: 59,       // alu op: a or b
dpc14_SRS: 362,      // alu op: logical right shift
dpc15_ANDS: 574,     // alu op: a and b
dpc16_EORS: 1666,    // alu op: a xor b (?)
dpc17_SUMS: 921,     // alu op: a plus b (?)
alucin: 910,         // alu carry in
notalucin: 1165,
"dpc18_#DAA": 1201,  // decimal related (inverted)
"dpc18_~DAA": 1201,   // automatic alias replacing hash with tilde
dpc19_ADDSB7: 214,   // alu to sb bit 7 only
dpc20_ADDSB06: 129,  // alu to sb bits 6-0 only
dpc21_ADDADL: 1015,  // alu to adl
alurawcout: 808,     // alu raw carry out (no decimal adjust)
notalucout: 412,     // alu carry out (inverted)
alucout: 1146,       // alu carry out (latched by phi2)
"#alucout": 206,
"~alucout": 206, // automatic alias replacing hash with tilde
"##alucout": 465,
"~~alucout": 465, // automatic alias replacing hash with tilde
notaluvout: 1308,    // alu overflow out
aluvout: 938,        // alu overflow out (latched by phi2)
"#DBZ": 1268,   // internal signal: not (databus is zero)
"~DBZ": 1268,    // automatic alias replacing hash with tilde
DBZ: 744,       // internal signal: databus is zero
DBNeg: 1200,    // internal signal: databus is negative (top bit of db) aka P-#DB7in
DBNeg: 1200,     // automatic alias replacing hash with tilde
"dpc22_#DSA": 725,   // decimal related/SBC only (inverted)
"dpc22_~DSA": 725,    // automatic alias replacing hash with tilde
dpc23_SBAC: 534,     // (optionalls decimal-adjusted) sb to acc
dpc24_ACSB: 1698,    // acc to sb
dpc25_SBDB: 1060,    // sb pass-connects to idb (bi-directionally)
dpc26_ACDB: 1331,    // acc to idb
dpc27_SBADH: 140,    // sb pass-connects to adh (bi-directionally)
dpc28_0ADH0: 229,    // zero to adh0 bit0 only
dpc29_0ADH17: 203,   // zero to adh bits 7-1 only
dpc30_ADHPCH: 48,    // load pch from adh
dpc31_PCHPCH: 741,   // load pch from pch incremented
dpc32_PCHADH: 1235,  // drive adh from pch incremented
dpc33_PCHDB: 247,    // drive idb from pch incremented
dpc34_PCLC: 1704,    // pch carry in and pcl FF detect?
dpc35_PCHC: 1334,    // pcl 0x?F detect - half-carry
"dpc36_#IPC": 379,   // pcl carry in (inverted)
"dpc36_~IPC": 379,    // automatic alias replacing hash with tilde
dpc37_PCLDB: 283,    // drive idb from pcl incremented
dpc38_PCLADL: 438,   // drive adl from pcl incremented
dpc39_PCLPCL: 898,   // load pcl from pcl incremented
dpc40_ADLPCL: 414,   // load pcl from adl
"dpc41_DL/ADL": 1564,// pass-connect adl to mux node driven by idl
"dpc42_DL/ADH": 41,  // pass-connect adh to mux node driven by idl
"dpc43_DL/DB": 863,  // pass-connect idb to mux node driven by idl
