Hardware requirements:

Best:
Console with 32k and ROM cartridge
-loads and runs smoothly from ROM

Second Best:
Console with 512k SAMS and DSSD floppy and XB or Editor/Assembler
-pre-loads entire demo from floppy to SAMS
-runs smoothly from SAMS RAM

Third Best:
Console with 32k and DSSD floppy and XB or Editor/Assembler
-Demo will run, but disk access between scenes will interrupt


Running:

Cartridge (32k required):
- Plug in the cartridge and select DEMO from the program list
- demo8.bin is a non-inverted 512k cartridge image for hardware or emulation
- ti99demo.rpk is a MAME/MESS cartridge for use with MAME or MESS

Disk with 512k SAMS and Editor/Assembler:
- Insert demo.dsk (DSSD) and run EA#5 "DSK1.SAMSDEMO"

Disk with 512k SAMS and Extended BASIC:
- Insert demo.dsk (DSSD) and start Extended BASIC
- LOAD program will offer a choice between 32k and 512k version, select 512k

Disk with 32k and Editor/Assembler:
- Insert demo.dsk (DSSD) and run EA#5 "DSK1.DEMOA"

Disk with 32k and Extended BASIC:
- Insert demo.dsk (DSSD) and start Extended BASIC
- LOAD program will offer a choice between 32k and 512k version, select 32k

Bonus:

For continuous run (such as at shows), leave Alpha Lock UP and the demo will repeat when it reaches the end.
