144 pictures of Speccy pixel goodness for your trusty old C128! No 64k needed (but DCR is recommended cause the music sounds better on new SID, which both Jason Page and Lman prefer! ;-) But we made sure 6581 works as well...

Choose whichever version suits you best, a single .d81 image, three .d71 images or six .d64 images. We recommend the .d81 version because it needs no disk swap! This has been tested on real HW and 1541 Ultimate with 1581/1571 beta firmware. Unfortunately it does not work on Pi1541 at this time, because it lacks c128 support for 2Mhz, Burst Mode and fast serial, which the Krill loader needs.

Press Shiftlock during slideshow or into to hold pictures and F1 to change music.

There may be some weird ass graphics bugs during fading that we cannot explain right now. Some of them are random and gone when you run the slideshow again (just press reset, it autoboots!). That VDC chip is just an odd beast...

DeeKay/Crest on 8/6/2021

P.S: TMR's C128 VDC demo is on the last disk of the .d71 and .d64 version! Farewell, Jason!

P.P.S.: GROOOOOOOVEN!!!!!!!