Larry & BSZ presents:
The VIC20 on the move
Streams animations from storage

-----

  System requirements:

1: Commodore VIC20 with +24K RAM
2: SD2IEC drive with VCPU-capable firmware¹

  For run: copy all the files to the new directory
on the SD card, go to that directory and type:

  LOAD"ba-vic20*",8 + [RETURN]
      or
  LOAD"med-vic20*",8 + [RETURN]
      or
  LOAD"still-vic20*",8 + [RETURN]
  RUN + [RETURN]

-----

¹ For usage, require VCPU-capable firmware.
  (See: FlexSD fw: bsz.amigaspirit.hu/vcpu)
