ErsKick ErsSnare ErsHihat ErsCymbal ErsBlipp ErsClaves ErsCowbell About ErsDrums

### ErsHihat (ErsDrums 1.2)

The hihat sound consists of a decaying metallic sound or noise burst passing through a highpass filter.

- NoiseType (metal/noise) selects if the hihat sound should be based on metallic sound or noise.
  Noise Type (0=metal, 1=noise)
- Cutoff (Hz) is the cutoff frequency of the highpass filter.
  Cutoff Frequency (0000=1000 Hz, 4000=9714 Hz, 8000=15000 Hz)
- Q (no unit) is the amount of resonance.
  Q (0000=0.7, 4000=5, 8000=10)
- ChDecay (ms) is the decay time of the amplitude of the noise burst for the closed hihat sound.
  Ch Decay (0000=10 ms, 4000=30 ms, 8000=50 ms)
- OhDecay (ms) is the decay time of the amplitude of the noise burst for the open hihat sound.
  Oh Decay (0000=10 ms, 4000=105 ms, 8000=200 ms)
- Gain (dB) is the output gain.
  Gain (00=-30 dB, 6A=0 dB, 7F=6 dB)