| # CYANPHASE SLIDE FLUTE
Type | Generator - Physical Modeling
Author | Edward L. Blake (CyanPhase), with some help from Jonathan Pak (Automaton)
Email | blakee@rovoscape.com
Description | An real-time implementation of a physical model slide flute based on Perry Cook's slide flute. Various settings are available to tweek the flute sound.
## PARAMETERS
Breath | Controls how much "breath" (noise) there is. Values are from 0.000 to 0.140.
Flow1: and Flow2: | Controls the ADSR envelopes for the flute, there are two of them, Flow1 controls mostly the breath.
Pressure | Amount of initial air pressure.
Feedback1 | Sets the amount of particle feedback that goes through the embouchure part of instrument, higher values sound very resonant however also distorted, lower values sound more "air-ish".
Feedback2 | Same as with Feedback1, however this is the amount of particle feedback going through the bore of the flute.
AttackAmt | A bit like a volume but not really, sets the initial "volume" going through the instrument, this is actually part of the ADSR envelopes
SustainAmt | Sets the sustained "volume" going through the instrument, this is actually part of the ADSR envelopes
RealVolume | Sets the output sound gain.
## STUFF
E-Mail: | blakee@rovoscape.com.

Copyright © 2000 Edward L. Blake