Geonik's Saturator

by George Nicolaidis

Description

The Saturator is a distortion that limits the input volume to the normal volume of Buzz (the volume that gives a full VU reading without clipping when sent directly to the Master) with a smoothly rounded input-output curve for soft transition to saturation.

What's new

Release 1 | Initial release

Usage

> P a r a m e t e r s

Drive | Pre-amplification of the input before distorting

Notes

No notes.

Contact Information

Author | George Nicolaidis
Email | geonik@egnatia.ee.auth.gr
HomePage | http://egnatia.ee.auth.gr/~geonik/home