ErsKick ErsSnare ErsHihat ErsCymbal ErsBlipp ErsClaves ErsCowbell About ErsDrums

### ErsBlipp (ErsDrums 1.2)

The blipp sound consists of a frequency sweep.

- StartFreq (Hz) is the initial frequency of the sweep.
  Sweep Start Frequency (0000=200 Hz, 4000=6300.1 Hz, 8000=10000 Hz)
- EndFreq (Hz) is the target frequency of the sweep.
  Sweep End Frequency (0000=20 Hz, 4000=132 Hz, 8000=200 Hz)
- Decay (ms) is the decay time of the amplitude of the sweep.
  Sweep Amplitude Decay (0000=10 ms, 4000=155 ms, 8000=300 ms)
- FreqDecay (ms) is the decay time of the frequency of the sweep.
  Sweep Frequency Decay (0000=10 ms, 4000=255 ms, 8000=500 ms)
- Gain (dB) is the output gain.
  Gain (00=-30 dB, 6A=0 dB, 7F=6 dB)