This is an update to the first recorder. This version should record silences properly,
so it should be easy to record loops. It also clips the output to avoid horrible garbage
pop sounds. You still need to watch your output levels so that it does not go to high or is
too soft. The volume that is going into the looper should be about what it takes to make the
VU meter go into the yellow/red range when the master volume is all the way up. If you
lower the master volume and your signal is still going into this range, then most likely it
is too loud. Likewise, you don't want the signal to be too soft. A good sampling takes up
most of the dynamic range.

The parameters: 
Volume: volume of signal (0-100%)
Length: length of time to record (in ticks)
Mode: Makes the recorder record, but not produce output
Trigger: Begins recording
