ErsKick ErsSnare ErsHihat ErsCymbal ErsBlipp ErsClaves ErsCowbell About ErsDrums

### ErsKick (ErsDrums 1.2)

The kick sound consists of two parts, a frequency sweep, and an initial thump.

- StartFreq (Hz) is the initial frequency of the sweep.
  Sweep Start Frequency (0000=150 Hz, 4000=305.6 Hz, 8000=400 Hz)
- EndFreq (Hz) is the target frequency of the sweep.
  Sweep End Frequency (0000=20 Hz, 4000=82.25 Hz, 8000=120 Hz)
- Decay (ms) is the decay time of the amplitude of the sweep.
  Sweep Amplitude Decay (0000=10 ms, 4000=255 ms, 8000=500 ms)
- FreqDecay (ms) is the decay time of the frequency of the sweep.
  Sweep Frequency Decay (0000=10 ms, 4000=155 ms, 8000=300 ms)
- Thump (%) is the mix between the thump sound and the sweep.
  Thump (0000=0 %, 4000=50 %, 8000=100 %)
- Gain (dB) is the output gain.
  Gain (00=-30 dB, 6A=0 dB, 7F=6 dB)