Frequency UnKnown Buzz Machine

Name: O-Delay

Type: Effect/Delay

Parameters: Left and Right settings for: Delay, Feedback, Input. Other settings are Dry Thru and X-Delay amount.

About: This effect is a slightly novel way of implementing a delay. For left and right channels, there are three parameters. 'Delay' sets the length of the delay in ticks/16. 'Feedback' sets the level of the delay output being fed back to the delay input. 'In' sets what level of the machine's input from other machines is fed into the delay. 'Dry Thru' sets the level of input that appears instantaneously at the output. 'X-Delay Amt' sets the level of output appearing on one delay that is fed back into the other delay.

Notes: The machine is incredibly versatile with this much routing customisation and can make sounds approaching reverb and guitar amp feedback rather than a delay sound.

Frequency UnKnown/Aybiss/Aaron Oxford

aybiss@hotmail.com / Aaron.Oxford@studentmail.newcastle.edu.au