ase development / buzz plugins
[asedev aEcho01] / name

[1.0] / revision
[effect] / type
[29.May.1999] / date of release

Description:
The [asedev aEcho01] machine is a very simple bandstyle echo effect. The user can choose the delay and the ratio he wants just by using the two parameters called "Delay" and "Ratio".

Parameters:
Delay: The parameter ranges from 0 to 0x3E7 (decimal: 999). Where a value of 0 is a delay of 0.0ms and a value of 0x3E7 is a delay of 999.0ms. The default delay is 100ms.
Ratio: The parameter ranges from 0 to 0x64 (decimal: 100). Where a value of 0 results in no echo and a value of 0x64 let the machine get freaky. The default ratio is 30.0%.

Contact:
For feedback and/or bug reports write to asedev@gmx.net

Licensing:
This software is FREEWARE. The author of this program cannot be held responsible for any damage this program may do to your system! Use it at your own risk!