REM --Sample configuration for a clean boot--

REM --For GUS ultrasound
DEVICE=C:\ULTRASND\ULTRINIT.SYS ULTRASND=240,7,7,11,7

DEVICE=C:\WINDOWS\HIMEM.SYS

REM --Sometimes EMM386 is needed but I rem it out till I need it.
REM DEVICE=C:\DOS\EMM386.EXE 

DOS=HIGH,UMB    
FILES=30
buffers =30 
DEVICEHIGH=C:\VIDEO\EANSI.SYS
