Glossary:

EG1     Envelope Generator 1 (Filter/Pitch)
EG2     Envelope Generator 2 (Volume)
LFO1    Low Frequency Oscillator 1 (Pitch/Volume/Filter)
LFO2    Low Frequency Oscillator 2 (Pitch)
FilterQ Filter Resonance

Explaination of EG's:

Delay:  The time before the attack, during which the envelope's
        level stays at 0.
Attack: The time during which the envelope's level fades from
        0 to peak.
Hold:   The time before the decay, during which the envelope's
        level stays at peak.
Decay:  The time during which the envelope's level fades from peak
        to the sustain level.
Sustain:The level at which the envelope stays before release.
Release:The time during which the envelope's level fades from sustain
        to 0.

        _
      /   \ __
____/          \

^    ^  ^^  ^  ^
|    |  ||  |  |
|    |  ||  |   - Release Time
|    |  ||   ---- Sustain Level
|    |  | ------- Decay Time
|    |    ------- Hold Time
|     ----------- Attack Time
 ---------------- Delay Time


