ErsKick ErsSnare ErsHihat ErsCymbal ErsBlipp ErsClaves ErsCowbell About ErsDrums

### ErsSnare (ErsDrums 1.2)

The snare sound consists of two parts, a decaying noise burst, and an initial thump.

- ThumpFreq (Hz) is the frequency of the thump sound.
  Thump Frequency (0000=150 Hz, 4000=305.6 Hz, 8000=400 Hz)
- ThumpDecay (ms) is the decay time of the amplitude of the thump sound.
  Thump Decay (0000=1 ms, 4000=6 ms, 8000=10 ms)
- NoiseDecay (ms) is the decay time of the amplitude of the noise burst.
  Noise Decay (0000=1 ms, 4000=26 ms, 8000=50 ms)
- Thump (%) is the mix between the thump sound and the noise burst.
  Thump (0000=0 %, 4000=50 %, 8000=100 %)
- Gain (dB) is the output gain.
  Gain (00=-30 dB, 6A=0 dB, 7F=6 dB)