  About the prologic:
  -------------------

  Authors:
  --------
  Ideas:  Gazbaby
  Coding:  Ynzn



  What's it?
  ----------
  It takes a stereo signal and splits it in four channels:  front, rear,
left and right.
  In fact, what it does is take two mono signals (the "normal" machine
input and the Auxbus input).  It lets you pan each of them left and right.
It also lets you pan them front and rear :).  You will hear nothing in
the middle of the panning (Zero Cool calls it "dead spot").  It's not
a bug.  The reason is that it's impossible to have the same signal coming
from both the front and rear at the same time (at least I don't know how
to do it... if only I had a prologic blablabla decoder...).

  If you don't have one of these, you will be only capable to pan left
and right.  In fact, Buzz lets you pan without any effect, so you'll find
this one useless...  :P

  Thank'yoes
  ----------
  To Gazbaby/Zero Cool, for all his support and... I don't know the word
in english... "peloteo".
  To Somee for his help and bugreports.
  To Arguru... Keep on coding!
  To Jose Luis Garcia "Agassi" (he wrote the algorithm of the "mediana").
  To Sine909... BuzzTrack is cool!
  To Jeskola (mr Tammelin)...  You're god!
  To mum and dad...  no, to mum and dad no.
  To all the ones I forgot... sorry!


					Ynzn